InS_StArT
yukodi.com
1.1
^Marvell Yukon Gigabit Ethernet Adapter,yukodi.com,0000P0
?If you want to use a specific adapter you have to select PCI Bus and Device Number. With CHECK_LINK the first adapter with a valid link will be used. Without parameter the first found adapter will be used.
*0IEMAP0(FRAME) Frame Type
?Ethernet_802.2 is now the default frame type for ODI drivers. Existing LANs may be using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
$00000P0 (BUSNUM) PCI Bus Number of selected adapter.
?Use yukodi -L to find all supported adapters. You have to specify DEVNUM too. If not specified, the driver will use the first adapter.
0
256
$00000P0 (DEVNUM) PCI Device Number of selected adapter.
?Use yukodi -L to find all supported adapters. You have to specify BUSNUM too. If not specified, the driver will use the first adapter.
0
32
!00000P0 (CONTYPE) Connection Type.
?You can force Speed and Duplex mode if auto-negotiation fails..
@AUTO
100FD
100HD
10FD
10HD
!00000P0 () Find first link.
?Select CHECK_LINK to load the driver to the first adapter with a valid link. This parameter will get ignored when BUSNUM or DEVNUM are specified.
CHECK_LINK
@
!00000P0 (RECEIVE BUFFERS) Number of receive buffers.
?Using more buffers might increase the performance but the driver needs more memory. The sum of receive and transmit buffers is limited to 6.
1
@2
3
4
5
!00000P0 (TRANSMIT BUFFERS) Number of transmit buffers.
?Using more buffers might increase the performance but the driver needs more memory. The sum of receive and transmit buffers is limited to 6.
1
@2
3
4
5
InS_EnD
